|  |  |  |
| --- | --- | --- |
|   |   | 1. Inventoried TWS components per TM
 |
|   |   | 1. Check the housing of the TWS for cracks, dents and dirt
 |
|   |   | 1. Ensure the eyecup and lens cap are present with no damage
 |
|   |   | 1. Inspect the control pad for cracks, dry rot and dirt
 |
|   |   | 1. Ensure objective focus ring turn smoothly to the end of travel
 |
|   |   | 1. Ensure that that the I/O port cap and lanyard are present, remove the cap and inspect for broken pins inside of the I/O port
 |
|   |   | 1. Inspect lenses for cracks, scratches and dirt, (if objective is damaged, do not ingest or inhale the crystals).
 |
|   |   | 1. Remove battery cassette from TWS and inspect for broken battery cassette and for corrosion on the cassette and inside of the battery compartment. Also inspect the spare battery cassette.
 |
|   |   | 1. Install batteries into battery cassette. Alignment tabs.
 |
|   |   | 1. Remove carrying handle and mount appropriate bracket if applicable.
 |
|   |   | 1. Loosen the torque limiting knob on the rail grabber
 |
|   |   | 1. Place TWS on M16A2/A4 or M4
 |
|   |   | 1. Place the TWS rail grabber completely on the picatinny rail.
 |
|   |   | 1. Mount the TWS to the weapon. Tighten down the torque limiting knob, two clicks while applying forward pressure.
 |
|   |   | 1. Turn TWS on. Wait for the start up period to end. Ensures there are no failures
 |
|   |   | 1. Select correct weapon reticle
 |
|   |   | 1. Adjusts the brightness of the screen to the individuals eye
 |
|   |   | 1. Select RET POL WHT/BLK
 |
|   |   | 1. Uncover the objective lens
 |
|   |   | 1. Adjust the objective focus ring to acquire a clear picture
 |
|   |   | 1. Perform a shuttered calibration
 |
|   |   | 1. Adjust Manual Gain
 |
|   |   | 1. Turn Auto gain on
 |
|   |   | 1. Select POL, users option WHT HOT/ BLK HOT
 |
|   |   | 1. Switch field of view
 |
|   |   | 1. Make any other needed optimization adjustments
 |
|   |   | 1. Instructor inspects the TWS for optimization.
 |
|   |   | 1. Place in Clip on configuration
 |
|   |   | 1. Put Remote key pad on weapon and connect
 |
|   |   | 1. Optimize TWS in Clip on mode
 |
|   |   | 1. 27. Instructor inspects the TWS for optimization.
 |
|   |   | 1. Turn TWS off and close lens cover.
 |
|   |   | 1. Loosen the torque-limiting knob.
 |
|   |   | 1. Remove the TWS from weapon
 |
|   |   | 1. Tighten torque limiting knob
 |
|   |   | 1. Remove battery cassette.
 |
|   |   | 1. Place full battery cassette into the storage container
 |
|   |   | 1. Place the TWS, properly, into the carrying case
 |